How to update your Charcot Circle

1. connect the module with a usb cable to your computer 
2. press simultaneously on SHIFT/PLAY/ENCODER 
3. download and launch HIdbootloader

« Device Attached.
Connecting… »

must be written on the screen.
4.import new firmware image (file menu)
5. program device 
6. reset device 

done. 

if you have any questions contact : info@eowave.com